|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Table S1** Chemical composition of hydrothermal gas along the Y-shaped fault system in the ETP. | | | | | | | | | | | | | | | | | |  |
| No. | Sample ID | Location | Data | Latitude | Longitude | T | Fault domain | N2 | O2 | | | CO2 | CH4 | | | Ar | He | Distance to fault |
| (°N) | (°E) | (°C) | (%) | | (%) | (%) | | | (%) | (%) | | (ppm) | (km) |
| 1 | QEL-1 | Qiaoelong | 09/2020 | 32.363 | 98.298 | 48.5 | YGXFS (YGF) | 72.8 | 0.65 | | | 25.6 | 0.33 | | | 0.61 | 809 | 4.3 |
| QEL-2 | Qiaoelong | 09/2020 | 32.363 | 98.298 | 48.5 | 75.3 | 0.78 | | | 22.9 | 0.34 | | | 0.67 | 589 | 4.3 |
| 2 | QR-1 | Quran | 09/2020 | 32.363 | 98.287 | 58.2 | 45.1 | 0.53 | | | 52.7 | 1.08 | | | 0.60 | 474 | 3.7 |
| QR-2 | Quran | 09/2020 | 32.363 | 98.287 | 58.2 | 45.5 | 0.58 | | | 52.3 | 1.09 | | | 0.54 | 498 | 3.7 |
| 3 | MR-1 | Marong | 09/2020 | 32.221 | 98.406 | 40.7 | 4.63 | 0.67 | | | 94.6 | 0.01 | | | 0.05 | 6.50 | -3.0 |
| MR-2 | Marong | 09/2020 | 32.221 | 98.406 | 40.7 | 9.54 | 2.10 | | | 88.2 | 0.01 | | | 0.10 | 6.20 | -3.0 |
| 4 | PW-1 | Queershan | 09/2020 | 31.956 | 98.860 | 33.8 | 2.12 | 0.56 | | | 97.3 | <0.01 | | | 0.02 | 0.1 | -15.3 |
| PW-2 | Queershan | 09/2020 | 31.956 | 98.860 | 33.8 | 3.70 | 0.84 | | | 95.4 | <0.01 | | | 0.03 | 0.1 | -15.3 |
| 5 | MN-1 | Maniganga | 09/2020 | 31.956 | 99.159 | 32.6 | 3.71 | 0.47 | | | 95.7 | 0.12 | | | 0.03 | 9.7 | -3.7 |
| MN-2 | Maniganga | 09/2020 | 31.956 | 99.159 | 32.6 | 3.58 | 0.52 | | | 95.8 | 0.07 | | | 0.02 | 9.4 | -3.7 |
| 6 | MDK-1 | Madake | 09/2020 | 31.826 | 99.439 | 39.4 | 11.7 | 0.64 | | | 87.1 | 0.34 | | | 0.15 | 44 | -2.3 |
| MDK-2 | Madake | 09/2020 | 31.826 | 99.439 | 39.4 | 10.8 | 0.49 | | | 88.1 | 0.43 | | | 0.15 | 37 | -2.3 |
| 7 | ZKX-1 | Zakexiang | 09/2020 | 31.902 | 99.640 | 28.4 | 8.35 | 0.86 | | | 89.5 | 1.19 | | | 0.07 | 121 | 15.0 |
| ZKX-2 | Zakexiang | 09/2020 | 31.902 | 99.640 | 28.4 | 6.58 | 0.62 | | | 92.1 | 0.63 | | | 0.06 | 111 | 15.0 |
| 8 | MYX-1 | Mayulongxi | 09/2020 | 31.788 | 99.699 | 40.0 | 22.2 | 0.36 | | | 32.5 | 44.7 | | | 0.26 | 1153 | 6.1 |
| MYX-2 | Mayulongxi | 09/2020 | 31.788 | 99.699 | 40.0 | 26.0 | 0.14 | | | 32.1 | 41.4 | | | 0.32 | 1442 | 6.1 |
| 9 | MYD-1 | Mayulongdong | 09/2020 | 31.786 | 99.699 | 46.3 | 35.4 | 0.48 | | | 59.7 | 4.00 | | | 0.44 | 2065 | 6.0 |
| MYD-2 | Mayulongdong | 09/2020 | 31.786 | 99.699 | 46.3 | 32.2 | 0.19 | | | 63.7 | 3.53 | | | 0.36 | 2087 | 6.0 |
| 10 | LM-1 | Laimajiake | 09/2020 | 31.688 | 99.778 | 39.4 | 90.2 | 8.62 | | | 0.48 | <0.01 | | | 0.70 | 25 | -2.6 |
| LM-2 | Laimajiake | 09/2020 | 31.688 | 99.778 | 39.4 | 90.2 | 8.76 | | | 0.35 | <0.01 | | | 0.72 | 34 | -2.6 |
| 11 | DDL-1 | Dingdalong | 09/2020 | 31.674 | 99.728 | 13.4 | 31.3 | 0.95 | | | 64.5 | 2.89 | | | 0.35 | 441 | 4.0 |
| DDL-2 | Dingdalong | 09/2020 | 31.674 | 99.728 | 13.4 | 33.3 | 1.38 | | | 62.0 | 2.96 | | | 0.36 | 459 | 4.0 |
| 12 | GYG-1 | Ganzi | 09/2020 | 31.583 | 100.043 | 15.5 | 10.4 | 1.00 | | | 83.9 | 4.66 | | | 0.07 | 158 | 2.3 |
| GYG-2 | Ganzi | 09/2020 | 31.583 | 100.043 | 15.5 | 15.0 | 2.53 | | | 78.0 | 4.33 | | | 0.13 | 150 | 2.3 |
| 13 | JX-01 | Jiaxicun | 09/2020 | 31.356 | 100.230 | 15.5 | 2.76 | 0.16 | | | 96.5 | 0.51 | | | 0.01 | 15 | -25.2 |
| JX-2 | Jiaxicun | 09/2020 | 31.356 | 100.230 | 15.5 | 3.46 | 0.57 | | | 95.3 | 0.68 | | | 0.03 | 15 | -25.2 |
| 14 | JY-1 | Jiayi | 09/2020 | 31.602 | 100.767 | 18.4 | YGXFS  (XSF) | 2.62 | 0.62 | | | 96.7 | <0.01 | | | 0.02 | 0.5 |  |
| JY-2 | Jiayi | 09/2020 | 31.602 | 100.767 | 18.4 | 3.11 | 0.84 | | | 96.0 | 0.01 | | | 0.03 | 0.5 | 23.4 |
| 15 | YD-1 | Yade | 09/2020 | 31.458 | 100.574 | 27.5 | 45.0 | 0.22 | | | 54.2 | 0.15 | | | 0.44 | 513 | 0 |
| YD-2 | Yade | 09/2020 | 31.458 | 100.574 | 27.5 | 47.2 | 0.59 | | | 51.6 | 0.16 | | | 0.50 | 537 | 0 |
| 16 | GK-1 | Geka | 09/2020 | 30.862 | 101.288 | 32.4 | 15.1 | 0.66 | | | 83.8 | 0.20 | | | 0.17 | 86.0 | 2.2 |
| GK-2 | Geka | 09/2020 | 30.862 | 101.288 | 32.4 | 15.1 | 0.71 | | | 83.8 | 0.19 | | | 0.17 | 86.0 | 2.2 |
| 17 | KM-1 | Kama | 09/2020 | 30.486 | 101.532 | 26.6 | 24.8 | 0.44 | | | 72.6 | 1.94 | | | 0.24 | 205 | 2.5 |
| KM-2 | Kama | 09/2020 | 30.486 | 101.532 | 26.6 | 24.0 | 0.89 | | | 73.0 | 1.91 | | | 0.25 | 176 | 2.5 |
| 18 | BM-1 | Bamei | 09/2020 | 30.532 | 101.618 | 51.2 | 3.03 | 0.46 | | | 96.1 | 0.37 | | | 0.02 | 3.5 | 0 |
| BM-2 | Bamei | 09/2020 | 30.532 | 101.618 | 51.2 | 4.26 | 0.92 | | | 94.3 | 0.47 | | | 0.03 | 3.6 | 0 |
| 19 | EDQ-1 | Erdaoqiao | 09/2020 | 30.087 | 101.950 | 40.8 | 4.14 | 0.29 | | | 95 | 0.07 | | | 0.04 | 5.9 | 0 |
| EDQ-2 | Erdaoqiao | 09/2020 | 30.087 | 101.950 | 40.8 | 6.38 | 0.81 | | | 93 | 0.09 | | | 0.06 | 7.6 | 0 |
| EDQ-18 | Erdaoqiao | 09/2015 | 30.088 | 102.242 | 41.0 | - | - | | | - | - | | | - | - | 0 |
| 20 | LTG-1 | Longtougou | 09/2020 | 29.979 | 101.957 | 71.9 | 2.21 | 0.55 | | | 97.1 | 0.08 | | | 0.02 | 0.8 | 0 |
| LTG-2 | Longtougou | 09/2020 | 29.979 | 101.957 | 71.9 | 7.08 | 2.12 | | | 90.6 | 0.11 | | | 0.07 | 0.7 | 0 |
| 21 | GD-1 | Guanding | 09/2020 | 29.952 | 101.961 | 76.0 | 6.81 | 1.76 | | | 91.0 | 0.36 | | | 0.06 | 4.5 | 0 |
| GD-2 | Guanding | 09/2020 | 29.952 | 101.961 | 76.0 | 5.86 | 1.36 | | | 92.4 | 0.34 | | | 0.05 | 4.8 | 0 |
| 22 | XX-1 | Xinxinxiang | 09/2015 | 29.754 | 102.060 | 46.0 | - | - | | | - | - | | | - | - | 0 |
| 23 | HM-12 | Hongmo | 09/2015 | 28.088 | 102.242 | 50.0 | ANFS | - | - | | | - | - | | | - | - | 5.7 |
| 24 | SQC-1 | Shangqingcun | 09/2020 | 31.614 | 104.349 | 19.3 | LMFS | 64.6 | 0.27 | | | 0.94 | 33.6 | | | 0.47 | 1249 | 5.9 |
| SQC-2 | Shangqingcun | 09/2020 | 31.614 | 104.349 | 19.3 | 64.3 | 0.21 | | | 0.99 | 33.8 | | | 0.57 | 1259 | 5.9 |
| 25 | JYG-1 | Jiyugou | 09/2020 | 31.627 | 103.771 | 26.0 | 93.2 | 0.14 | | | 5.69 | 0.12 | | | 0.71 | 186 | 0.9 |
| 26 | MCG-1 | Muchengou | 09/2020 | 31.525 | 103.003 | 43.2 | 96.9 | 0.11 | | | 1.41 | 0.27 | | | 1.27 | 793 | -50.6 |

*Note:* YGXFS, Yushu-Ganzi-Xianshuihe fault system; YGF, Yushu-Ganzi fault; XSF, Xianshuihe fault; ANFS, Anninghe fault system; LMFS, Longmenshan fault system.

**Table S2** Isotopic composition of hydrothermal gas along the Y-shaped fault system in the ETP.

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| No. | Sample ID | 4He/20Ne | Xmb | Rm/Raa | Rc/Rac | CO2/3Hed | δ13CCH4 | δ13CCO2 | Mantle He | Carbon inventoryf | | |
| (109) | (‰) | (‰) | (%) | M (%) | L (%) | S (%) |
| 1 | QEL-1 | 50 | 192 | 0.13 | 0.13 | 1.8 | - | -8.8 | 1.32 | - | - | - |
| QEL-2 | 52 | 199 | 0.13 | 0.13 | 2.2 | - | -8.2 | 1.32 | - | - | - |
| 2 | QR-1 | 50 | 192 | 0.12 | 0.12 | 6.9 | -37.7 | -7.9 | 1.19 | - | - | - |
| QR-2 | 49 | 188 | 0.12 | 0.12 | 6.5 | -30.0 | -6.9 | 1.19 | - | - | - |
| 3 | MR-1 | 36 | 138 | 0.37 | 0.37 | 287 | - | -4.6 | 4.33 | 0.7 | 84.1 | 15.2 |
| MR-2 | 34 | 130 | 0.41 | 0.41 | 253 | - | -4.0 | 4.83 | 0.7 | 86.1 | 13.2 |
| 4 | PW-1 | - | - | - | - | - | - | -4.1 | - | - | - | - |
| PW-2 | 1.7 | 6.5 | 0.36 | 0.24 | - | - | -3.7 | 2.81 | - | - | - |
| 5 | MN-1 | 95 | 364 | 0.17 | 0.17 | 423 | - | -4.8 | 1.85 | 0.5 | 83.6 | 15.9 |
| MN-2 | 99 | 380 | 0.18 | 0.18 | 412 | - | -4.9 | 1.98 | 0.5 | 83.3 | 16.2 |
| 6 | MDK-1 | 42 | 161 | 0.04 | 0.03 | 420 | - | -7.0 | 0.17 | 0.5 | 76.3 | 23.2 |
| MDK-2 | 30 | 115 | 0.04 | 0.03 | 544 | -19.4 | -7.1 | 0.14 | 0.3 | 76.1 | 23.6 |
| 7 | ZKX-1 | 220 | 844 | 0.12 | 0.12 | 45 | -38.8 | -3.1 | 1.24 | 4.4 | 86.2 | 9.4 |
| ZKX-2 | 255 | 978 | 0.12 | 0.12 | 50 | -29.7 | -3.6 | 1.24 | 4.0 | 84.9 | 11.1 |
| 8 | MYX-1 | 397 | 1523 | 0.04 | 0.04 | 5.2 | -49.0 | -8.4 | 0.24 | - | - | - |
| MYX-2 | 374 | 1435 | 0.04 | 0.04 | 4.1 | -48.9 | -8.9 | 0.24 | - | - | - |
| 9 | MYD-1 | 433 | 1661 | 0.04 | 0.04 | 5.3 | -26.8 | -6.2 | 0.24 | - | - | - |
| MYD-2 | 431 | 1654 | 0.04 | 0.04 | 5.5 | -25.8 | -5.3 | 0.25 | - | - | - |
| 10 | LM-1 | 2.3 | 8.8 | 0.45 | 0.38 | 0.4 | - | -5.9 | 4.50 | - | - | - |
| LM-2 | 2.0 | 7.7 | 0.41 | 0.32 | 0.2 | - | -5.9 | 3.77 | - | - | - |
| 11 | DDL-1 | 92 | 353 | 0.08 | 0.08 | 14 | -24.4 | -4.9 | 0.72 | - | - | - |
| DDL-2 | 91 | 349 | 0.07 | 0.07 | 14 | -22.2 | -4.8 | 0.59 | - | - | - |
| 12 | GYG-1 | 184 | 706 | 0.18 | 0.18 | 21 | -26.2 | -3.7 | 1.99 | - | - | - |
| GYG-2 | 200 | 767 | 0.21 | 0.21 | 18 | -25.8 | -4.0 | 2.37 | - | - | - |
| 13 | JX-01 | 153 | 587 | 0.13 | 0.13 | 360 | -32.8 | -0.7 | 1.36 | 0.5 | 97.3 | 2.2 |
| JX-2 | 164 | 629 | 0.12 | 0.12 | 385 | -32.9 | -1.2 | 1.24 | 0.5 | 95.6 | 3.9 |
| 14 | JY-1 | 3.7 | 14 | 0.61 | 0.58 | 2399 | - | -0.2 | 7.02 | 0.1 | 99.3 | 0.6 |
| JY-2 | 3.4 | 13 | 0.65 | 0.62 | 2226 | - | -2.3 | 7.53 | 0.1 | 92.3 | 7.6 |
| 15 | YD-1 | 75 | 288 | 0.21 | 0.21 | 3.7 | - | -2.6 | 2.35 | - | - | - |
| YD-2 | 60 | 230 | 0.21 | 0.21 | 3.3 | - | -3.1 | 2.34 | - | - | - |
| 16 | GK-1 | 58 | 223 | 0.10 | 0.10 | 73 | - | -5.4 | 0.95 | 2.7 | 79.9 | 17.4 |
| GK-2 | 58 | 223 | 0.12 | 0.12 | 60 | - | -5.3 | 1.20 | 3.3 | 79.8 | 16.9 |
| 17 | KM-1 | 58 | 223 | 0.24 | 0.24 | 11 | -18.1 | -4.4 | 2.71 | - | - | - |
| KM-2 | 59 | 226 | 0.25 | 0.25 | 12 | -20.4 | -4.8 | 2.84 | - | - | - |
| 18 | BM-1 | 36 | 138 | 0.22 | 0.21 | 922 | - | -3.9 | 2.43 | 0.2 | 86.8 | 13.0 |
| BM-2 | 33 | 127 | 0.23 | 0.22 | 842 | - | -4.5 | 2.55 | 0.2 | 84.8 | 15.0 |
| 19 | EDQ-1 | 17 | 65 | 1.76 | 1.77 | 66 | - | -4.6 | 22.0 | 3.0 | 82.3 | 14.7 |
| EDQ-2 | 21 | 81 | 1.77 | 1.78 | 49 | - | -2.6 | 22.1 | 4.0 | 88.2 | 7.8 |
| EDQ-18 | 17 | 65 | 2.34 | 2.37 | - | - | -4.9 | 29.4 | - | - | - |
| 20 | LTG-1 | 9.1 | 35 | 1.72 | 1.74 | 502 | - | -2.6 | 21.6 | 0.4 | 91.0 | 8.6 |
| LTG-2 | 9.0 | 35 | 1.87 | 1.90 | 491 | - | -4.8 | 23.5 | 0.4 | 83.7 | 15.9 |
| 21 | GD-1 | 34 | 130 | 2.27 | 2.28 | 64 | -23.6 | -3.7 | 28.3 | 3.1 | 85.2 | 11.7 |
| GD-2 | 32 | 123 | 2.18 | 2.19 | 63 | - | -3.6 | 27.2 | 3.2 | 85.5 | 11.3 |
| 22 | XX-14 | 526 | 2020 | 0.94 | 0.94 | - | - | -8.9 | 11.5 | - | - | - |
| 23 | HM-12 | 235 | 903 | 0.07 | 0.07 | - | - | -8.1 | 0.63 | - | - | - |
| 24 | SQC-1 | 153 | 587 | 0.02 | 0.02 | 0.3 | -47.5 | -15.6 | 0.00 | - | - | - |
| SQC-2 | 154 | 591 | 0.01 | 0.01 | 0.7 | -47.1 | -17.3 | 0.00 | - | - | - |
| 25 | JYG-1 | 151 | 579 | 0.03 | 0.03 | 7.8 | - | -5.2 | 0.10 | - | - | - |
| 26 | MCG-1 | 27 | 104 | 0.04 | 0.03 | 0.4 | - | - | 0.13 | - | - | - |

a Measured 3He/4He ratios of samples (Rm/Ra) are divided by the 3He/4He ratio of air (1.39 × 10−6).

b Xm = (4He/20Ne)measured/(4He/20Ne)air × *ß*Ne/*ß*He, where Xm is air contamination factor and the air saturated water (ASW) normalized 4He/20Ne ratio taken as 0.26; *ß* represents Bunsen solubility coefficients for He and Ne in pure water (*ß*Ne/*ß*He = 1.22, Holocher et al., 2002), assuming a groundwater recharge temperature of 15 °C (see details in Hilton, 1996).

c Rc/Ra is the air-corrected He isotope ratio = [(Rm/Ra × Xm) – 1] / (Xm – 1).

d CO2/3He is calculated based on air-corrected 3He content.

e Mantle He proportion (*f* mantle ) = [(Rc / Ra)measured − (R / Ra)crust] / [(R / Ra)mantle − (R / Ra)crust], where (R/Ra)mantle and(R/Ra)crust are 3He/4He ratios of mantle (8 Ra, Graham, 2002) and crust (0.02 Ra, Ozima and Podosek, 2002), respectively.

f Mantle (M), carbonate (CAR) and organic matter (ORG) proportions in total carbon inventory are calculated using the following the approach (Sano and Marty, 1995): ƒM + ƒCAR+ ƒORG = 1; (13C / 12C)sam = (13C / 12C)M × ƒM + (13C / 12C)CAR × ƒCAR + (13C / 12C)ORG × ƒORG; 1 / (12C / 3He)sam = ƒM / (12C / 3He)M + ƒCAR / (12C / 3He)CAR + ƒORG / (12C / 3He)ORG, where ƒM, ƒCAR and ƒORG are the fraction contribution by M, CAR and ORG end-members to the total CO2 inventory, respectively; sam is the observed ratio of samples. he assumed endmembers compositions are reported: δ13CCO2 = −6.5 ± 2.5‰, CO2/3He = 2 × 109 for M, δ13CCO2 = 0 ± 2‰, CO2/3He = 1013 for CAR; δ13CCO2 = −30 ± 10‰, CO2/3He = 1013 for ORG (Sano and Marty, 1995).

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Table S3** Calculation of the mantle fluid flux and using reference parameters in hydrothermal gases along the YGXFS and ANFS. | | | | | | | | | | | |
| Sample ID | 4He in spring watera | Original 4He mantle concentrationa | Crust thickness, *H*crustb | Porosity, Øc | Bulk rock density, ρsc | 4He production rate, P(4He) | U contentd | Th contentd | 3He flow rate | Total 3He flux | Mantle CO2 flux |
| (cm3 STP g-1 H2O) | (cm3 STP g-1 H2O) | (km) | (kg m-1 s-1) | (g cm-3) | (cm3 STP g-1 yr-1) | (ppm) | (ppm) | (mm yr-1) | (mol m-2 yr-1) | (mol m-2 yr-1) |
| QEL-1 | 4.54E-06 | 5.99E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 32 | 1.11E-12 | 2.23E-03 |
| QEL-2 | 3.30E-06 | 4.37E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 44 | 1.12E-12 | 2.23E-03 |
| QR-1 | 2.76E-06 | 3.27E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 52 | 1.01E-12 | 2.03E-03 |
| QR-2 | 2.90E-06 | 3.46E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 50 | 1.02E-12 | 2.04E-03 |
| MR-1 | 3.46E-08 | 1.50E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| MR-2 | 3.30E-08 | 1.59E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| PW-2 | 4.38E-10 | 1.23E-11 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| MN-1 | 5.24E-08 | 9.70E-10 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| MN-2 | 5.08E-08 | 1.00E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| ZKX-1 | 6.90E-07 | 8.56E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 208 | 1.06E-12 | 2.11E-03 |
| ZKX-2 | 6.33E-07 | 7.87E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 227 | 1.06E-12 | 2.11E-03 |
| LM-1 | 1.24E-07 | 5.60E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 |  |  |  |
| LM-2 | 1.65E-07 | 6.25E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 |  |  |  |
| DDL-1 | 3.10E-06 | 2.23E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 36 | 5.39E-13 | 1.08E-03 |
| DDL-2 | 3.22E-06 | 1.91E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 44 | 5.39E-13 | 1.19E-03 |
| GYG-1 | 1.16E-06 | 2.31E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 125 | 1.60E-12 | 3.20E-03 |
| GYG-2 | 1.10E-06 | 2.61E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 132 | 1.88E-12 | 3.75E-03 |
| JX-1 | 8.99E-08 | 1.22E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| JX-2 | 8.99E-08 | 1.11E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| JY-1 | 2.35E-09 | 1.65E-10 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| YJ-2 | 2.62E-09 | 1.98E-10 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| YD-1 | 3.00E-06 | 7.05E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 48 | 1.86E-12 | 3.72E-03 |
| YD-2 | 3.14E-06 | 7.34E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 46 | 1.85E-12 | 3.71E-03 |
| GK-1 | 4.81E-07 | 4.58E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 298 | 8.49E-13 | 1.70E-03 |
| GK-2 | 4.81E-07 | 5.79E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 299 | 1.03E-12 | 2.06E-03 |
| KM-1 | 1.14E-06 | 3.09E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 128 | 2.13E-12 | 4.26E-03 |
| KM-2 | 9.79E-07 | 2.78E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 149 | 2.22E-12 | 4.45E-03 |
| BM-1 | 2.03E-08 | 4.93E-10 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| BM-2 | 2.08E-08 | 5.32E-10 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| ZGC01\* | 6.94E-08 | 1.35E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| EDQ-1 | 3.71E-08 | 8.13E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| EDQ-2 | 4.79E-08 | 1.06E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| EDQ04\* | 1.15E-07 | 3.58E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 1797 | 3.19E-11 | 6.38E-02 |
| LTG-1 | 5.29E-09 | 1.14E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| LTG-2 | 4.63E-09 | 1.09E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| LTG02\* | 2.95E-08 | 5.96E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| GD-1 | 3.08E-08 | 8.74E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| GD-2 | 3.29E-08 | 8.94E-09 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | - | - | - |
| GD02\* | 2.07E-07 | 7.01E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 1039 | 3.61E-11 | 7.23E-02 |
| EHY01\* | 2.17E-07 | 3.78E-08 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 794 | 1.50E-11 | 3.00E-02 |
| CK02\* | 5.31E-06 | 5.70E-07 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 30 | 8.61E-12 | 1.72E-02 |
| GYH01\* | 1.45E-04 | 7.74E-07 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 1 | 5.51E-13 | 1.10E-03 |
| HM01\* | 1.42E-04 | 1.31E-06 | 60 | 0.09 | 2.78 | 8.53E-13 | 3.38 | 15.53 | 1 | 8.28E-13 | 1.66E-03 |

*Note*: Hot springs with Rc/Ra < 0.05 are not used for calculation of mantle fluid flux along the YGXFS.

a Detail about calculation of 4He contents in spring water and original 4He mantle concentration are described in Zhang et al. (2022).

b The average of crust thickness (*H*crust) in the eastern Tibet Plateau is cited from Jiang et al. (2015).

c Porosity (Ø) and bulk rock density (*ρ*s) are cited from Hu (1985).

d U and Th contents in rocks are from 523 rock samples in study region.

-: 3He flow rate is not considered due to low helium content and significant atmospheric contamination (Xm < 10 or < 4) for gas samples that is suspicious in causing large uncertainty of calculating mantle fluid flow rate.

\* Literature data are from Xu et al. (2022) along the YGXFS and ANFS.

**Table S4** The compiled He-isotope data for geothermal fluids and distance along different strike-slip faults fault in the world.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Sample ID | Latitude (°N) | Longitude (°E) | Sample type | 4He/20Ne | R/Ra | Rc/Ra | Distance from fault (km) | Reference |
| **Itoigawa-Shizuoka tectonic line (IST)** | | |  |  |  |  |  | a |
| Kan1 | 36.489 | 137.912 | W | 1.06 | 3.0 | 3.6 | - |
| Sas2 | 36.448 | 137.981 | W | 0.67 | 0.9 | 0.8 | - |
| Kus3 | 36.437 | 138.074 | W | 0.52 | 1.7 | 2.4 | - |
| Azu4 | 36.311 | 137.826 | W | 0.87 | 3.1 | 4 | - |
| Ana5 | 36.333 | 138.002 | G | 11.4 | 0.7 | 0.7 | - |
| Uts6 | 36.248 | 138.001 | W | 2.04 | 2.5 | 2.7 | - |
| Tob7 | 36.185 | 138.085 | W | 0.75 | 0.8 | 0.7 | - |
| Ten8 | 36.141 | 138.006 | W | 0.33 | 1.0 | 1.1 | - |
| Cho9 | 36.165 | 137.948 | W | 4.14 | 1.6 | 1.7 | - |
| Myo10 | 36.19 | 137.83 | W | 24.7 | 2.1 | 2.1 | - |
| Shi11 | 36.077 | 138.091 | G | 16.3 | 4.7 | 4.8 | - |
| Kam12 | 36.052 | 138.114 | G | 20.6 | 5.3 | 5.4 | - |
| Tat13 | 35.966 | 137.992 | G | 93.3 | 0.8 | 0.8 | - |
| Mid14 | 36.090 | 138.002 | G | 29 | 1.1 | 1.1 | - |
| Kob15 | 35.878 | 138.317 | G | 297 | 4.6 | 4.6 | - |
| Shi16 | 35.877 | 138.257 | G | 184 | 6.0 | 6 | - |
| Oji17 | 35.808 | 138.34 | G | 2150 | 4.9 | 4.9 | - |
| Muk18 | 35.784 | 138.379 | G | 419 | 3.9 | 3.9 | - |
| Mah19 | 35.882 | 137.919 | G | 111 | 1.6 | 1.6 | - |
| Oya20 | 35.762 | 138.32 | W | 11.8 | 5.3 | 5.4 | - |
| Kof21 | 35.662 | 138.57 | W | 33 | 4.0 | 4.1 | - |
| Tog22 | 35.651 | 138.41 | W | 0.52 | 0.7 | 0.4 | - |
| Nis23 | 35.554 | 138.307 | G | 17.6 | 2.9 | 2.9 | - |
| Mom24 | 35.624 | 138.357 | G | 1.82 | 2.5 | 2.9 | - |
| Jik25 | 35.505 | 138.394 | W | 235 | 6.8 | 6.8 | - |
| Fun26 | 35.294 | 138.421 | W | 0.34 | 1.3 | 2.2 | - |
| Jya27 | 35.933 | 138.105 | W | 0.33 | 1.2 | 1.8 | - |
| Kas28 | 35.587 | 138.056 | W | 39.7 | 1.4 | 1.4 | - |
| Toy29 | 35.322 | 137.929 | G | 1210 | 2.4 | 2.4 | - |
| Hon30 | 34.879 | 137.426 | G | 649 | 0.5 | 0.5 | - |
| Soe31 | 35.108 | 137.575 | W | 8.8 | 0.9 | 0.9 | - |
| Shr32 | 35.124 | 137.29 | W | 8.7 | 0.8 | 0.8 | - |
| War33 | 35.079 | 137.118 | G | 2620 | 0.3 | 0.3 | - |
| Kuz34 | 36.494 | 137.75 | W | 3.69 | 2.5 | 2.6 | - |
| Nan35 | 36.494 | 137.724 | W | 0.41 | 0.9 | 0.7 | - |
| **Southeastern Korean Peninsula (SeKP)** | | |  |  |  |  |  | b |
| G1 | 35.785 | 129.325 | W | 0.4 | 1.09 | 1.2 | - |
| G2 | 35.930 | 129.206 | W | 38 | 5.51 | 5.54 | - |
| U1 | 35.553 | 129.126 | W | 0.4 | 0.84 | 0.55 | - |
| U3 | 35.593 | 129.116 | W | 0.7 | 0.7 | 0.55 | - |
| U4 | 35.570 | 129.337 | W | 0.3 | 0.96 | 0.87 | - |
| U5a | 35.624 | 129.223 | W | 12 | 0.07 | 0.05 | - |
| U5b | 35.624 | 129.223 | W | 2.8 | 0.17 | 0.09 | - |
| U8a | 35.538 | 129.256 | W | 17 | 4.84 | 4.9 | - |
| U8b | 35.538 | 129.256 | W | 38 | 5.66 | 5.69 | - |
| P1a | 36.159 | 129.278 | W | 19 | 1.38 | 1.39 | - |
| P1b | 36.159 | 129.278 | W | 33 | 1.27 | 1.27 | - |
| P3 | 36.195 | 129.327 | W | 0.5 | 1.34 | 1.68 | - |
| B1a | 35.162 | 129.166 | W | 24 | 0.34 | 0.33 | - |
| B1b | 35.162 | 129.166 | W | 39 | 0.31 | 0.3 | - |
| B2a | 35.221 | 129.081 | W | 37 | 0.34 | 0.34 | - |
| B2b | 35.221 | 129.081 | W | 25 | 0.46 | 0.46 | - |
| **North Anatolian fault (NAF)** | | | | | | | | |
| M03 | ‐ | ‐ | G | 13 | 0.35 | 0.34 | -20.1 | c |
| M05 | ‐ | ‐ | G | 81 | 0.26 | 0.25 | -26.6 |
| M07 | ‐ | ‐ | G | 4.19 | 0.52 | 0.48 | -69.8 |
| M09 | ‐ | ‐ | G | 0.38 | 0.95 | ‐ | -92.23 |
| M11‐1 | ‐ | ‐ | G | 111 | 0.28 | 0.28 | -35.4 |
| M11‐2 | ‐ | ‐ | G | 23.3 | 0.29 | 0.28 | -35.3 |
| M12‐R1 | ‐ | ‐ | G | 7.9 | 2.74 | 2.81 | 18.5 |
| M13 | ‐ | ‐ | G | 0.57 | 0.84 | 0.63 | -13.63 |
| M14 | ‐ | ‐ | G | 484 | 0.59 | 0.59 | -13.63 |
| M15 | ‐ | ‐ | G | 81 | 0.66 | 0.66 | 8.4 |
| M16 | ‐ | ‐ | G | 59 | 0.61 | 0.61 | -2 |
| M65 | ‐ | ‐ | G | 68 | 0.97 | 0.97 | 49.9 |
| M66 | ‐ | ‐ | G | 2050 | 1.32 | 1.32 | -22.81 |
| M01 | ‐ | ‐ | W | 42.6 | 0.65 | 0.65 | -15.4 |
| M02 | ‐ | ‐ | W | 0.43 | 0.83 | 0.33 | -49.0 |
| M04‐1 | ‐ | ‐ | W | 44.8 | 0.29 | 0.28 | -11.2 |
| M04‐2 | ‐ | ‐ | W | 43.7 | 0.27 | 0.26 | -10.9 |
| M06 | ‐ | ‐ | W | 1.81 | 0.28 | 0.13 | -34.4 |
| M08 | ‐ | ‐ | W | 9.31 | 0.68 | 0.66 | -89.7 |
| M10‐1 | ‐ | ‐ | W | 9.82 | 1.07 | 1.07 | 1 |
| M10‐2 | ‐ | ‐ | W | 4.1 | 0.88 | 0.87 | 0.5 |
| M12‐3 | ‐ | ‐ | W | 4.61 | 2.14 | 2.22 | -19.9 |
| M17 | ‐ | ‐ | W | 0.47 | 0.87 | 0.6 | -30.4 |
| M50 | ‐ | ‐ | W | 28.1 | 0.56 | 0.55 | 9.2 |
| M51 | ‐ | ‐ | W | 7.5 | 0.54 | 0.52 | 9.0 |
| M52 | ‐ | ‐ | W | 0.31 | 0.95 | ‐ | 24.0 |
| M53 | ‐ | ‐ | W | 0.34 | 0.88 | ‐ | 23.7 |
| M54 | ‐ | ‐ | W | 0.37 | 0.82 | ‐ | 22.1 |
| M56 | ‐ | ‐ | W | 0.25 | 0.99 | ‐ | 6.2 |
| M59 | ‐ | ‐ | W | 0.32 | 0.94 | ‐ | 7.1 |
| M62 | ‐ | ‐ | W | 0.35 | 0.87 | ‐ | 15.3 |
| M63 | ‐ | ‐ | W | 0.66 | 0.42 | ‐ | 15.6 |
| M64 | ‐ | ‐ | W | 0.95 | 0.53 | 0.29 | 64.1 |
| M67 | ‐ | ‐ | W | 1.93 | 4.22 | 4.85 | 0 |
| M68‐1 | ‐ | ‐ | W | 0.33 | 1.25 | ‐ | 0 |
| M68‐2 | ‐ | ‐ | W | 0.34 | 1.36 | ‐ | 0 |
| **Karakoram fault (KKF)** | | | | | | | | |
| ZP02 | 31.131 | 80.719 | G | 22.6 | 2.225 | 2.23 | -0.2 | d |
| ZZD12-1 | 31.091 | 80.571 | G | 166 | 0.032 | 0.03 | -15.9 |
| ZZD09 - 2 | 31.062 | 80.546 | G | 355 | 0.030 | 0.03 | -19.7 |
| ZGR15 | 31.372 | 80.489 | G | 1374 | 0.032 | 0.03 | -0.6 |
| ZGR09 | 31.446 | 80.405 | G | 1053 | 0.024 | 0.02 | -1.6 |
| ZGR06 | 31.923 | 80.166 | G | 2620 | 0.026 | 0.03 | 2.2 |
| ZGR05 | 32.243 | 79.877 | G | 141 | 0.032 | 0.03 | -0.6 |
| K13G | 33.559 | 78.141 | W | 133 | 0.020 | 0.02 | -33.7 |
| K13C | 33.360 | 78.324 | G | 3212 | 0.023 | 0.02 | -37.1 |
| K13P | 33.223 | 78.327 | G | 5935 | 0.009 | 0.01 | -48.8 |
| ZGR08 | 32.363 | 80.361 | G | 519 | 0.192 | 0.19 | 47.7 |
| **San Andreas fault (SAF)** | | | | | | | | |
| CUY-01 | ‐ | ‐ | W | 3.41 | 0.78 | 0.5 | 17.7 | e |
| CUY-02 | ‐ | ‐ | W | 1.78 | 0.4 | 0.3 | 16.9 |
| CUY-03 | ‐ | ‐ | W | 0.38 | 0.97 | 0.2 | 11.9 |
| CUY-04 |  |  | W | 1.01 | 0.93 | 1 | 11.9 |
| CUY-05 | ‐ | ‐ | W | 2.65 | 0.52 | 0.47 | 15.5 |
| CUY-06 |  |  | W | 0.75 | 1.04 | 1 | 10 |
| CUY-07 |  |  | W | 1.35 | 1.02 | 1 | 9.5 |
| CUY-08 |  |  | W | 0.59 | 1.17 | 1 | 11.2 |
| CUY-11 | ‐ | ‐ | W | 1.17 | 0.82 | 0.49 | 21.0 |
| CUY-12 | ‐ | ‐ | W | 0.41 | 0.94 | 0.09 | 11.4 |
| CUY-09 | ‐ | ‐ | W | 3.47 | 0.68 | 0.64 | 0.19 |
| CUY-10 | ‐ | ‐ | W | 3.98 | 3 | 3.1 | 0.58 |
| CUYU-01 |  |  | W | 1.92 | 1.62 | 1.33 | 0.13 |
| CUYU-02 |  |  | W | 3.58 | 2.4 | 2.3 | 0.28 |
| CUYU-03 | ‐ | ‐ | W | 2.11 | 2.07 | 2.16 | 0.1 |
| CUYU-04 | ‐ | ‐ | W | 6.64 | 3.47 | 3.52 | 0.29 |
| CUYU-05 | ‐ | ‐ | W | 0.74 | 0.93 | 0.1 | -0.84 |
| CUYU-06 | ‐ | ‐ | W | 0.80 | 1.27 | 1.02 | 17.7 |
| **Red River fault (RRF)** | | | | | | | | |
| Glc1 | 23.998 | 104.433 | G | 14.63 |  | 0.09 | 153 | f |
| Lcc2 | 23.639 | 104.412 | G | 0.53 |  | 0.47 | 121 |
| Pzh3 | 23.429 | 104.152 | G | 2.39 |  | 0.10 | 86 |
| Bsp4 | 23.423 | 104.146 | G | 13.02 |  | 0.04 | 85 |
| Rsc5 | 23.531 | 104.055 | G | 2.20 |  | 0.07 | 88 |
| Cjz6 | 23.354 | 103.981 | G | 37.92 |  | 0.09 | 68 |
| Ehg7 | 23.298 | 103.968 | G | 251.91 |  | 0.10 | 63 |
| Yd8 | 23.311 | 103.942 | G | 222.62 |  | 0.11 | 62 |
| Xf9 | 23.322 | 103.796 | G | 216.85 |  | 0.16 | 53 |
| Bhq10 | 22.940 | 103.861 | G | 167.18 |  | 0.19 | 27 |
| Mp11 | 22.914 | 103.489 | G | 6.05 |  | 0.47 | -1 |
| Mlz12 | 22.931 | 103.429 | G | 37.48 |  | 0.46 | -4 |
| Mpy13 | 22.902 | 103.457 | G | 24.00 |  | 0.43 | -4 |
| Ddp14 | 22.990 | 103.362 | G | 38.40 |  | 0.39 | -2 |
| Fcl15 | 22.998 | 103.115 | G | 53.19 |  | 0.09 | -10 |
| Slc116 | 22.704 | 103.287 | G | 11.37 |  | 0.11 | -33 |
| Nx17 | 22.533 | 103.028 | G | 98.11 |  | 0.05 | -64 |
| Pe18 | 22.653 | 103.044 | G | 23.65 |  | 0.05 | -51 |
| Yx19 | 22.762 | 102.755 | G | 43.91 |  | 0.10 | -50 |
| Js20 | 23.356 | 102.942 | G | 83.49 |  | 0.14 | 18 |
| Lcc21 | 23.430 | 102.973 | G | 57.46 |  | 0.06 | 27 |

Abbreviations: G = gas sample; W = water sample. Literature data are from: a, Umeda et al. (2013); b, Lee et al. (2019); c, Doǧan et al. (2009); d, Klemperer et al. (2022); e, Kulongoski et al. (2013); f, Wang et al. (2020).

**References**

Doǧan, T., Sumino H., Nagao, K., Notsu, K., Tuncer, M.K., & Çelik, C. (2009). Adjacent releases of mantle helium and soil CO2 from active faults: Observations from the Marmara region of the North Anatolian Fault zone, Turkey. Geochemistry, Geophys. Geosystems 10, Q11009.

Hu, X. (1985). Physical state of fluid in High Temperature Geothermal Reservoir and Well-hydrothermodynamic analysis and calculation. Acta Geol. Sin. 1, 74–86.

Jiang, G., Xu, X., Chen, G., Liu, Y., Fukahata, Y., Wang, H., Yu, G., Tan, X., & Xu, C. (2015). Geodetic imaging of potential seismogenic asperities on the Xianshuihe-Anninghe-Zemuhe fault system, southwest China, with a new 3-D viscoelastic interseismic coupling model. J. Geophys. Res. Solid Earth 120, 1855–1873.

Klemperer, S., Zhao, P., Whyte, C., Darrah, T., Crossey, L., Liu, T.Z., Winn, C., Hilton, D., & Ding, L. (2022). Limited underthrusting of India below Tibet: 3He/4He analysis of thermal springs locates the mantle suture in continental collision. Proc. Natl. Acad. Sci. 119, e2113877119.

Kulongoski, J.T., Hilton, D.R., Barry, P.H., Esser, B.K., Hillegonds, D., & Belitz, K. (2013). Volatile fluxes through the Big Bend section of the San Andreas Fault, California: Helium and carbon-dioxide systematics. Chem. Geol. 339, 92–102.

Lee, H., Kim, H., Kagoshima, T., Park, J. O., Takahata, N., & Sano, Y. (2019). Mantle degassing along strike-slip faults in the Southeastern Korean Peninsula. Sci. Rep. 9, 15334.

Wang, Y., Liu, Y., Zhao, C., Li, Q., Zhou, Y., & Ran H. (2020). Helium and carbon isotopic signatures of thermal spring gases in southeast Yunnan, China. J. Volcanol. Geotherm. Res. 402, 106995.

Xu, S., Guan, L., Zhang, M., Zhong, J., Liu, W., Xie, X., Liu, C., Takahata, N., & Sano, Y. (2022). Degassing of deep-sourced CO2 from Xianshuihe-Anninghe fault zones in the eastern Tibetan Plateau. Sci. China Earth Sci. 65, 139–155.

Zhang, M., Liu, W., Guan, L., Sano, Y., Takahata, N., Li, Y., Zhou, X., Chen, Z., Cao, C.H., Zhang, L., Lang, Y.-C., Liu, C.-Q., & Xu, S. (2022). Vigorous Mantle Degassing in the Southeast Tibetan Plateau Margin Evidenced by. Geophys. Res. Lett. 49, e2022GL098228.

Umeda, K., Asamori, K., & Kusano, T. (20.13). Release of mantle and crustal helium from a fault following an inland earthquake. Applied Geochemistry 37134-141